ipmiutil ver 2.93
isensor: version 2.93
-- BMC version 2.40, IPMI version 2.0 
 ID  | SDRType | Type            |SNum| Name             |Status| Reading
0001 | Compact | Event Log       | 72 | SEL              | Absent | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
0002 | Compact | Platform Securi | 73 | Intrusion        | OK   | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
000b | Full    | Fan             | 30 | Fan1A            | OK   | 1680.00 RPM 	| Thresholds| lo-noncr 840.00 | lo-crit 720.00  | Mon May 15 08:34:34 2014
000c | Full    | Fan             | 31 | Fan1B            | OK   | 1560.00 RPM 	| Thresholds| lo-noncr 840.00 | lo-crit 720.00  | Mon May 15 08:34:34 2014
000d | Full    | Fan             | 32 | Fan2A            | OK   | 3120.00 RPM 	| Thresholds| lo-noncr 840.00 | lo-crit 720.00  | Mon May 15 08:34:34 2014
000e | Full    | Fan             | 33 | Fan2B            | OK   | 2880.00 RPM 	| Thresholds| lo-noncr 840.00 | lo-crit 720.00  | Mon May 15 08:34:34 2014
000f | Full    | Fan             | 34 | Fan3A            | OK   | 3000.00 RPM 	| Thresholds| lo-noncr 840.00 | lo-crit 720.00  | Mon May 15 08:34:34 2014
0010 | Full    | Fan             | 35 | Fan3B            | OK   | 2880.00 RPM 	| Thresholds| lo-noncr 840.00 | lo-crit 720.00  | Mon May 15 08:34:34 2014
0011 | Full    | Fan             | 36 | Fan4A            | OK   | 2280.00 RPM 	| Thresholds| lo-noncr 840.00 | lo-crit 720.00  | Mon May 15 08:34:34 2014
0012 | Full    | Fan             | 37 | Fan4B            | OK   | 2160.00 RPM 	| Thresholds| lo-noncr 840.00 | lo-crit 720.00  | Mon May 15 08:34:34 2014
0013 | Full    | Fan             | 38 | Fan5A            | OK   | 2280.00 RPM 	| Thresholds| lo-noncr 840.00 | lo-crit 720.00  | Mon May 15 08:34:34 2014
0014 | Full    | Fan             | 39 | Fan5B            | OK   | 2160.00 RPM 	| Thresholds| lo-noncr 840.00 | lo-crit 720.00  | Mon May 15 08:34:34 2014
0015 | Full    | Temperature     | 04 | Inlet Temp       | OK   | 21.00 C 	| Thresholds| hi-crit 47.00 | hi-noncr 42.00 | lo-noncr 3.00 | lo-crit -7.00  | Mon May 15 08:34:34 2014
0016 | Compact | Watchdog_2      | 71 | OS Watchdog      | OK   | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
0017 | Compact | Voltage         | 23 | VCORE PG         | OK | 	| Entity ID 3.1 (Processor), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
0018 | Compact | Voltage         | 19 | 3.3V PG          | OK | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
0019 | Compact | Voltage         | 1a | 5V PG            | OK | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
001a | Compact | Cable/Interconn | 50 | USB Cable Pres   |  _  | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
001b | Compact | Entity Presence | 70 | Dedicated NIC    | Present | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
001c | Compact | Cable/Interconn | 51 | VGA Cable Pres   |  _  | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
001d | Compact | Entity Presence | 49 | Presence         | OK*  | 	| Entity ID 11.2 (Add-in card), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
001e | Compact | Entity Presence | 40 | Presence         | OK*  | 	| Entity ID 3.1 (Processor), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
001f | Compact | Voltage         | 25 | PLL PG           | OK | 	| Entity ID 3.1 (Processor), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
0020 | Compact | Voltage         | 27 | 1.1V PG          | OK | 	| Entity ID 0.1 (unspecified), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
0021 | Compact | Voltage         | f6 | BP1 5V PG        | OK | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
0022 | Compact | Entity Presence | 43 | Presence         | OK*  | 	| Entity ID 10.2 (Power supply), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
0023 | Compact | Voltage         | 2b | VSA PG           | OK | 	| Entity ID 3.1 (Processor), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
0024 | Compact | Voltage         | 1e | MEM VDDQ PG      | OK | 	| Entity ID 3.1 (Processor), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
0025 | Compact | Cable/Interconn | 4c | LCD Cable Pres   |  _  | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
0026 | Compact | Voltage         | 20 | VTT PG           | OK | 	| Entity ID 3.1 (Processor), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
0027 | Compact | Entity Presence | 48 | Presence         | Present | 	| Entity ID 11.3 (Add-in card), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
0028 | Compact | Processor       | 60 | Status           | ProcPresent | 	| Entity ID 3.1 (Processor), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:34 2014
0029 | Compact | Fan             | 75 | Fan Redundancy   | Redundant | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
002c | Compact | Cable/Interconn | 64 | Riser Config Err |  _  | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
002d | Compact | Voltage         | 28 | 1.5V PG          | OK | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
002e | Compact | Voltage         | 2c | PS2 PG Fail      | OK | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
002f | Compact | Voltage         | 2d | PS1 PG Fail      | OK | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0030 | Compact | Voltage         | 14 | MEM VTT PG       | OK | 	| Entity ID 3.1 (Processor), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0031 | Compact | Entity Presence | 42 | Presence         | OK*  | 	| Entity ID 10.1 (Power supply), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0032 | Compact | Critical Interr | 90 | PCIe Slot1       | OK   | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0033 | Compact | Critical Interr | 91 | PCIe Slot2       | OK   | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0034 | Compact | Critical Interr | 92 | PCIe Slot3       | OK   | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0035 | Compact | Critical Interr | 93 | PCIe Slot4       | OK   | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0036 | Compact | Memory          | c0 | A                | OK   | 	| Entity ID 32.1 (Memory device ), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0039 | Compact | Board           | fa | vFlash           | OK   | 	| Entity ID 12.1 (Front panel bd), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
003a | Compact | Battery         | 65 | CMOS Battery     | OK   | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
003b | Compact | Entity Presence | 54 | Presence         | OK*  | 	| Entity ID 26.1 (Disk Drive Bay), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
003c | Full    | Current         | 6a | Current 1        | OK   | 0.20 A 	| Thresholds | Mon May 15 08:34:35 2014
003d | Full    | Current         | 6b | Current 2        | OK   | 0.20 A 	| Thresholds | Mon May 15 08:34:35 2014
003e | Full    | Voltage         | 6c | Voltage 1        | OK   | 228.00 V 	| Thresholds | Mon May 15 08:34:35 2014
003f | Full    | Voltage         | 6d | Voltage 2        | OK   | 228.00 V 	| Thresholds | Mon May 15 08:34:35 2014
0040 | Compact | Power Supply    | 74 | PS Redundancy    | NotAvailable | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0041 | Compact | Power Supply    | 62 | Status           | Present | 	| Entity ID 10.1 (Power supply), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0042 | Compact | Power Supply    | 63 | Status           | Present | 	| Entity ID 10.2 (Power supply), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0043 | Full    | Current         | 77 | Pwr Consumption  | OK   | 84.00 W 	| Thresholds| hi-crit 1456.00 | hi-noncr 1330.00  | Mon May 15 08:34:35 2014
0044 | Compact | OEM(c0)         | 76 | Power Optimized  | Asserted | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0045 | Compact | OEM(c9)         | f4 | SD1              |  _  | 	| Entity ID 11.3 (Add-in card), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0046 | Compact | OEM(c9)         | f5 | SD2              |  _  | 	| Entity ID 11.3 (Add-in card), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0047 | Compact | OEM(c9)         | 78 | Redundancy       |  _  | 	| Entity ID 11.3 (Add-in card), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0048 | Compact | Memory          | 01 | ECC Corr Err     | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0049 | Compact | Memory          | 02 | ECC Uncorr Err   | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
004a | Compact | Critical Interr | 03 | I/O Channel Chk  | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
004b | Compact | Critical Interr | 04 | PCI Parity Err   | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
004c | Compact | Critical Interr | 05 | PCI System Err   | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
004d | Compact | Event Log       | 06 | SBE Log Disabled | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
004e | Compact | Event Log       | 07 | Logging Disabled | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
004f | Compact | System Event    | 08 | Unknown          | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0050 | Compact | Processor       | 0a | CPU Protocol Err | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0051 | Compact | Processor       | 0b | CPU Bus PERR     | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0052 | Compact | Processor       | 0c | CPU Init Err     | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0053 | Compact | Processor       | 0d | CPU Machine Chk  | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0054 | Compact | Memory          | 11 | Memory Spared    | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0055 | Compact | Memory          | 12 | Memory Mirrored  | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0056 | Compact | Memory          | 13 | Memory RAID      | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0057 | Compact | Memory          | 14 | Memory Added     | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0058 | Compact | Memory          | 15 | Memory Removed   | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
0059 | Compact | Memory          | 16 | Memory Cfg Err   | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
005a | Compact | Memory          | 17 | Mem Redun Gain   | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:35 2014
005b | Compact | Critical Interr | 18 | PCIE Fatal Err   | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
005c | Compact | Critical Interr | 19 | Chipset Err      | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
005d | Compact | OEM(c1)         | 1a | Err Reg Pointer  | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
005e | Compact | Memory          | 1b | Mem ECC Warning  | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
005f | Compact | Memory          | 1c | Mem CRC Err      | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0060 | Compact | Memory          | 1d | USB Over-current | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0061 | Compact | System Firmware | 1e | POST Err         | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0062 | Compact | Version Change  | 1f | Hdwr version err | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0063 | Compact | Memory          | 20 | Mem Overtemp     | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0064 | Compact | Memory          | 21 | Mem Fatal SB CRC | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0065 | Compact | Memory          | 22 | Mem Fatal NB CRC | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0066 | Compact | Watchdog_1      | 71 | OS Watchdog Time | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0067 | Compact | Memory          | 26 | Non Fatal PCI Er | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0068 | Compact | Memory          | 27 | Fatal IO Error   | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0069 | Compact | Memory          | 28 | MSR Info Log     | Unknown | 	| Entity ID 34.1 (BIOS), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
006a | Compact | Drive Slot      | a0 | Drive 0          | Unused   Faulty | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
006b | Compact | Cable/Interconn | e0 | Cable SAS A      |  _  | 	| Entity ID 26.1 (Disk Drive Bay), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
006c | Compact | Cable/Interconn | e1 | Cable SAS B      |  _  | 	| Entity ID 26.1 (Disk Drive Bay), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
006d | Compact | Cable/Interconn | e2 | Cable SAS C      |  _  | 	| Entity ID 26.1 (Disk Drive Bay), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
006e | Compact | Cable/Interconn | e3 | Cable SAS D      |  _  | 	| Entity ID 26.1 (Disk Drive Bay), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
006f | Compact | Cable/Interconn | 58 | Power Cable      |  _  | 	| Entity ID 26.1 (Disk Drive Bay), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0070 | Compact | Cable/Interconn | 59 | Signal Cable     |  _  | 	| Entity ID 26.1 (Disk Drive Bay), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0071 | Compact | Voltage         | 66 | PFault Fail Safe | Absent | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0072 | Compact | Battery         | 68 | ROMB Battery     | OK   | 	| Entity ID 11.2 (Add-in card), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0073 | Compact | Battery         | 69 | ROMB Battery     | OK   | 	| Entity ID 11.4 (Add-in card), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0074 | Compact | Cable/Interconn | 4d | Riser 1 Presence |  _  | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0075 | Compact | Cable/Interconn | 4e | Riser 2 Presence |  _  | 	| Entity ID 7.1 (System board), Capab: arm=auto thr=none evts=state | Mon May 15 08:34:36 2014
0077 | Full    | Temperature     | 0e | Temp             | OK   | 66.00 C 	| Thresholds| hi-crit 83.00 | hi-noncr 77.00 | lo-noncr 8.00 | lo-crit 3.00  | Mon May 15 08:34:36 2014
ipmiutil sensor, completed successfully

